From Bottom to Top the Outputs are:

+15V

-15V

+3.3V

LCD Power

LCD Signal

DC/DC Converter

…the Inputs are:

Charger

Key